Adapter

A Trident (model #01.029.5) 6.0” FNPT (female national pipe thread) x 5.0” MNH (male national hose thread) chrome plated brass, internal lug adapter will be installed. A zinc die-cast strainer shall be installed on the MNH end of the adapter. The strainer shall be held in place with a retainer clip for easy removal if needed. The adapter will meet or exceed all NFPA 1901 standards and will be hydrostatically pressure tested up to 600psi. Where applicable, Trident Equalizer™ pressure reliving type threads will be provided on the NH threads.