Adapter

A Trident (model #01.141.0) 1.00” FNPT (female national pipe thread) x 0.75” MGHT (male garden hose thread) chrome plated brass, external hex adapter will be installed. The adapter will meet or exceed all NFPA 1901 standards and will be hydrostatically pressure tested up to 600psi.