Adapter

A Trident (model #01.053.0) 1.50” FNPT (female national pipe thread) x 1.50” MNH (male national hose thread) chrome plated brass, internal lug adapter will be installed. The adapter will meet or exceed all NFPA 1901 standards and will be hydrostatically pressure tested up to 600psi. Where applicable, Trident Equalizer™ pressure reliving type threads will be provided on the NH threads.