BLACK FOLDING STEP

A Trident Model (#24.005.15) black folding step will be installed. The step will be NFPA 1901 design compliant for load, size requirements and slip resistance. The step will be constructed of a die cast allow, with a black non-corrosive coating applied. The slip resistance step surface will be constructed with a black tread. The step surface shall be lighted with a super bright LED light to a 2-foot candles per square foot. The step will be mounted with two (2) 5/16” (0.3125”) bolts.